**ESS responses to review recommendations from Nov 2017**

**Questions to ESS (to be answered before the end of November 2017)**

1. Confirm that there is no need for deionized water in the low temperature water system (8 degrees).
2. Check if 50 degrees water input could be used for target cooling.

**Response from ESS**

1. Not to use deionized water in the CWL loop has been a requirement in all steering documents in ESS since 2016. This requirement has been verified with internal stakeholders in ESS during the last year. There has not come up any new information that would question this requirement.

2. The requirement 50 degrees or lower (45-50) is communicated and confirmed with Target Division.